2

2.1

2.2

2.3

2.4

2.5

-25 -20 -15 -10 -5 0

ϕ_2-ϕ_1 Μ1/3 deg stripsΝ η p_t = 2.5 GeV

Track Bending in CMS

For |η|>1.4 the total ∫B×dl decreases with η. Tracks are less bent for larger |η|. This limits the strip length to Δη≈0.1.

Constraints for the trigger granularity