New Simple Muon Geometry

IMVERS = 904 or 906

MS 1-4: 2 x 4 layers: 10 mm gas / 1 mm Al MF 0-4: 4 or 6 layers: 5 mm gas / 22 mm honeycomb

MF0 and MF1 form double first station MF0 can be desabled by commenting out the titles

Other flags for muon matching: KINE: IKINE = -74

PKINE(1) - number of ISAJET events others: like for normal muon fit (see CMSIM manual)