G. Wrochna CMS Muon Meeting, 30.03.94

OPTIMIZATION

OF THE FORWARD MUON SYSTEM

Momentum resolution curves for LOI have been obtained assuming 2 "superlayers" per stations. Now we consider CSC model shown above.

setup layers / MF1 layers / MF2−4 σ (rφ) layer effic. old 2 2 100 μm 95 % new 2 x 4 4 70 μm 80 %

We will vary parameters of the new design and observe behaviour of the momentum resolution.

Al honeycomb gas 22 mm

5 mm