GEOMETRY OF THE MUON SYSTEM

IMVERS parameter of the card CMSV:

• 900 - average medium • 901 - 2 layers/station, 30cm apart

1mm Al, 1cm gas, 1mm Al

• 902 - 10 layers/station, equaly spaced • 910, 911, 912 - as above, with dead spaces

in preparation

IMVERS=-1 equivalent to 900

Recomended geometry setup:

VERS mom.fit trig.study

ICVERS 9 9 ITVERS -1 0 IEVERS -1 -1 IHVERS -1 -1 IMVERS 901 900 IFVERS 0 0

Geometry version IxVERS=-1 in case of

•HCAL is created by HGEOM •TRAK & ECAL are created by MGEOM