CSC Cluster Logic

A track fires 3-4 strips but sub-strip resolution is needed ! The half-strip resolution can be obtained in the following way:

1 0 - left half-strip 0 1 - right half-strip 0 0 - no hit

Q2 Q1 Q3

+ - + - - + - + threshold

η strip width σ_{ρ φ}

2.0 16 mm 800 μm

⇒ dp/p < 30 % @ p_t= 100 GeV

2.5 6 mm 300 μm