CSC Local Charged Track Logic

A local charged track (LCT) is determined by a pattern of hit strips in a given chamber.

E.g. ± 25 mrad range ⇒ 44 patterns / strip 6 layers • 10 strips / chip ⇒ 1 mm^2 of 0.8 μm VLSI