Muon Trigger Data Readout

Recording some trigger data is necessary for

• calibration • monitoring • histograming

- trigger logic status - rejected events

E.g. in case of CSC there are the following possibilities:

• row trigger data

- right after discriminators on individual strips and wires

• mother board input - LCT etc. • mother board output - primitives (vector per station) • track finder output

Serguei Khabarov khabarov@cernvm.cern.ch from Dubna is willing to look at the problem.