CSC track segments and η/ϕ ambiguities

Signals from wire cards (η) and strip cards (ϕ) are sent to the motherboard. Here they should be combined into one track segment. However, 2μ crossing the same chamber cause ambiguities. There is no clear idea how to solve them by the CSC itself.

strip card wire card mother board