RPC strips are 6× shorter than CSC strips.

Simple coincidence of CSC strip & wire with an RPC strip can solve ambiguities.

Solving ambiguities in CSC locally with RPC

Implementation seems to be cheap & easy ⇒ let’s build it. However CSC and RPC efficiencies are multiplied. Therefore it should be kept as an "emergency option" and used only in case of problems with backgroung rates.