Drift Tube Muon Trigger

Every muon station has 3 meantimers serving 4 layers each.

Each meantimer provides an information about:

position in 1.25 mm units angle in 60 mrad units Information from meantimers in a given station is combined by "correlator" and delivered to the full track logic.