CMS Muon Trigger

DESIGN OBJECTIVES

1. Excellent performance in wide p_t range:

2-4 GeV ⇔ 100 GeV μ E-loss limit DAQ limit

2. Large safety margins:

- to account for inaccuracy of simulations, and uncertainty of extrapolations from lower energies - to be ready for surprises