80

90

100

1 10 10^2 10^3 p_t (GeV)

efficiency (%)

Domains of the two trigger subsystems

High p_t region in the barrel

High p_t muons have frequent showers, which can overload the meantimers of the DT system.

This cause a drop of one station efficiency above 200 GeV. It can be partially recovered by other stations.

RPC logic always chose the highest p_t pattern.

μ 300 GeV

RD 5