CMS Trigger Meeting at Bad Aussee, G. Wrochna, RPC Muon T rigger for CMS, pa ge 2 June 18, 1994

CMS Muon Trigger

Tasks:

- muon recognition 10-20 l on a m way

- bunch crossing a ssignment Dt < 25 ns - programmable p_t cut 4-100 GeV

Additional requirem ents:

- no dead time pipe line mode - high speed < 1 ms for decision - output rate acca ptable for event fi lter ~ a few kHz - high acceptance every track crosses ‡3 stations - redundancy to deal with noise, pileup, etc. - on board mainten ance remote testing and programming