CMS Muon System

Why 4 muon stations ? - full geometrical acceptance

every track crosses > 3 stations - pattern recognit ion

(ambiguities, noise , punchthrough)

- redundancy to de al with muon radiat ion p 20 GeV

m 300 GeV