Choice of the reference station

Additional adavantage of choice of MS2: the same station is the reference for low and high p_t.

MS2 ref. MS1 ref. MS3 ref. MS4 ref.

The number of interconnections in φ is minimised if MS2 is chosen as the reference station.

high p_t low p_t

MS1 MS2 MS3 MS4

MS1 MS2 MS1’

MS2’