CMS Muon Trigger

How to deal with geometrical inefficiencies?

• ensure that every track crosses ≥3 planes • require all 4 planes to be fired, but • consider dead areas as "fired" • don’t accept "tracks" with >1 such artificial

• • • • • •••• •••• •• •

high p_t μ

"ghost"