Simulation of muon secondaries in RPC

iron

5 cm air gap RPC