RPC System in CMS

1656 two-gap RPC’s 3400 m^2 of total area ~200 000 channels

The numbers are big!