Δt (98% of events) < 15 ns

rate capability: barrel: ε>98% for 100 Hz/cm^2 endcap: - 1500 Hz/cm^2

clusters: av. cluster size < 2 strips < 1% ev. of > 4 strip clusters

Δϕ (endcap) = 5/16°

Δϕ (barrel) = 5/16°

Δz (barrel) ≈ 1 m

Δη (endcap) ≈ 0.1

4 stations (>80%) ≥3 stations (100%)

RPC performance RPC geometry

bunch crossing identification (25 ns)

expected hit rate: barrel: < 20 Hz/cm^2 endcap: < 700 Hz/cm^2

momentum measurement up to 50-100 GeV