Features of the RPC System

NO AMBIGUITIES - ϕ, η, t given by the same signal

PRECISE TIMING - adjustable gate < 25 ns - time based background rejection

BUNCH CROSSING DETERMINATION - straightforward - safe

MOMENTUM MEASUREMENT FOR TRIGGER - programmable algorithm - easy to adopt for actual conditions

READOUT OF FULL DETECTOR INFORMATION - useful for resolving ambiguities

in off-line pattern recognition ( strips are 6× shorter than those of CSC )