Muon Induced Secondaries

Realistic simulation requires simulation of bremsstrahlung and direct pair production down to 1 MeV and δ−rays even lower, which is extremaly time consuming. Possible solution for electrons is to apply cuts dependent on the distance to a chamber, e.g.:

100 keV last 1 mm of Al (chamber wall) 1 MeV last 5 mm of iron 10 MeV 5 - 50 mm of iron 100 MeV anywhere else Photons need more care because they do not lose energy.

Laszlo Urban from GEANT Team works on the problem.

μ 300 GeV

RD 5