RPC Trigger - Background Simulation

RPC trigger logic simulated by MTRIG

CMS detector and shielding geometry:

CMS Status Report, May ’94

Input:

neutron and gamma fluxes: FLUKA, CMS TN/94-241 RPC intrinsic noise = 1 Hz/cm^2 (RD5 experience) electronics noise = 100 Hz/channel (arbitrary number)

Statistics:

2 000 000 GEANT/CMSIM muons 70 000 000 random n/γ hits

~ 1 week of CPU