1 10 10^2

10^3

10^4

10^5

10^6

1 10 10^2 p_t^{cut} ΜGeVΝ trigger rate ΜHzΝ

|η|Λ2.5

3 kHz

L=10^{32}

4.5

L=10^{33}

10

L=10^{34}

25

Criteria for Single Muon Triggers

Trigger criteria can be based on cut purity s :

s trigger performance > 50% good 10 - 50 % limited < 10% poor

Let’s assume 3 kHz rate allowed for a single muon trigger.

The trigger should have a good performance down to the lowest p_t accessible for muons.