RPC trigger acceptance for |η|<0.81

Assumed dead area: 2cm on the sides, 4cm at the ends

low pt - MB1, MB1’, MB2, MB2’ high pt - MB1, MB2, MB3, MB4

low pt high pt 3/4 4/4 3/4 4/4

baseline 72.7 51.2 87.9 48.4 compromised 72.7 51.2 89.9 46.4 fully slanted 71.0 50.6 86.9 45.2

Conclusions: - fully slanted solution is the worst - compromised is 2% better than baseline for 3/4 at high pt