Compatibility of Muon Triggers in CMS

Information delivered by muon triggers should be compatible with each other and with calorimeters:

η φ ±p_t "quality"

[0.35] [20°] 1+5 bits

CSC: DT: RPC: HCAL:

- bits with the same meaning for all the systems

The most significant bits of η, φ, and p_t should have the same meaning

for all the systems.