CSC Trigger

Probability of real and fake local triggers

MF1 prototype recently tested in the CMS test beam: "endcap configuration", behind calorimeter,

π, μ: 50-300 GeV, B=0-3 T, measured with ADC and TDC.

The data will be passed through the CSC trigger simulation.

P0 prototype will be tested in August with electronics providing 1/2 strip resolution for trigger.