RPC Acceptance in the Barrel

Coincidence of 3 out of 4 RPC planes is required: @ low p_t: MS1, MS1’, MS2, MS2’ solid line @ high p_t: MS1, MS2, MS3, MS4 dashed line

The lowest possible effective p_t cut ≈ 3.6 GeV

0 20 40 60 80 100

2 3 4 5 6 7 8 p_t (GeV)

RPC trigger acceptance (%)

MS1,1’,2,2’

MS1,2,3,4 μ- |η| < 0.15