RPC Low p_t Trigger Acceptance

0 0.01

0.02

0.03

0.04

0.05

0.06

0.07

0.08

260 280 300 320 340 360 380 400 420 wheel lenght (cm) dead Δη

10 12 14 16 18 20 cm gap

3 out of 4 RPC planes in MS1,2 required 2 x 4 cm dead RPC border current design

5 equal wheels 3 equal wheels

CONCLUSIONS:

making the wheels longer - does not help very much reducing the gap width - every cm counts