RPC Low p_t Trigger Acceptance

Δη_1 Δη_2

dead areas:

MS 3

MS 4

@ p_t> 6 GeV: MS 1, 2, 3, 4 used

≥3 out of 4 everywhere

@ 3.6 < p_t< 6 GeV: MS 1, 1’, 2, 2’ used

≥3 out of 4 everywhere except Δη_1 and Δη_2

MS 1

MS 1’

MS 2’ MS 2

In the current design the total dead area is 2 (Δη_1+Δη_2) = 0.15 i.e. 0.15 / 4.8 = 3 % of single muon acceptance and 6 % of two muon acceptance.