Cathode Strip Chamber Trigger

TIME:

OR of 6 planes of wires first pulse gives t_0 but ≥4 planes out of 6 must be fired t_{drift}^{max} = 40 ns ⇒ σ(t_0) < 3 ns

POSITION:

cluster center in every plane of strips Δx = 1/2 strip width

ANGLE:

local charged track (LCT) determined by pattern of fired half-strips in a given station

MOMENTUM:

combination of LCT’s from all stations strips wires