Solving ambiguities in CSC globally with RPC • CSC delivers strip and wire track segments separately • Sector Processor performs extrapolation and matching

of track segments in each projection independently

• Two projections are combined by the Global Trigger • Ambiguities are solved by comparing with tracks in RPC

RPC PACT processor gives unambiguous muon track position with precision: Δη≈0.1 Δϕ=2.5°