Muon Chamber Trigger Logic

strips wires

Q2 Q1 Q3 + - + - - + - + threshold

CSC

Comparators give 1/2-strip resol.

Hit strips of 6 layers form a vector.

μ 4 3 2 1

1 2 3 4

Drift Tubes

Meantimers recognize tracks and form vector / quartet.

Correlator combines them into one vector / station.

track segment muon station 4

muon station 3

muon station 2

muon station 1

2 x extrapolation threshold

3 track segment pairs are combined to one track string ϕ2 - ϕ1